* What is coercion in C?
* Size of character literal in C?
* What is trigraph characters?

Combination of 3 char which generate a single character

* Max arguments type main fun can take

int main(int argc, char\*argv[], char \*env[])

ans – 3

* What is segmentation fault

Trying to access memory which is not allocated

* BigEndian and LittleEndian

BigEndian is when msb is at lower address

LittleEndian is when msb is at higher address

* Segment: it is memory allocated for the program
* Floating values are stored using Mantissian technique

1st bit = sign

8th bit = exp

23nd bit = mantissa

0 000 0101.011 = 1.01011 x E2 =

* Wchar\_t = 2 to 65536

Size = 2;

Char 1-256

Size = 1;

* Name Mangling
* VTABLE?

Virtual table

* VPTR?

Virtual tables are pointed

* RTTI

Runtime type identification

typeid() operator

typeid(obj).name()